#### ULi Integrated Driver of AGP, IDE Cache, Ultra IDE, FIR, Audio, USB, M5228, M5281, M5287,M5288, M5289, M5461, M7101 and IRQ ####

   This integrated driver integrates 
1. AGP driver V2.14 for Win2K/WinXP with M1563,  V2.30 for WinXP/2003/x64 , V2.14Win98SE/WinME
2. IDE Cache Utility 1.06 for Win95 OSR2.1/Win98/Win98SE/WinME.
3. Mini-IDE driver 1.5.1.0 for Win2K/WinXP(WHQL).
4. FIR driver 1.150 for Win98(WHQL)/Win98SE(WHQL). FIR driver 1.141 for WinME(WHQL) 
   FIR driver 2.01 for Win2K(WHQL)/WinXP(WHQL). 
5. Audio M5451 WDM driver 5.12.01.5260 for Win98SE/WinME(WHQL)/Win2K(WHQL)/WinXP(WHQL).
6. Audio M5455 WDM driver 5.12.01.7006 for Win98SE/WinME/Win2K/WinXP(WHQL), 5.12.01.7005 for x64.
   Audio M5455 WDM driver for Vista(tested on Vista beta Build 5320)
7. Memory Stick driver 1.32.1018 for Win98SE/WinME,and 1.32.1030 for Win2000/WinXP.
8. SD/MMC driver 1.10.1018 for Win98SE/WinME,and 1.10.1040 for Win2000/WinXP.
9. LAN driver 3.50 for Win98/Win98SE/WinME/Win2K(WHQL)/2003/WinXP(WHQL)/x64(WHQL).
   LAN driver 3.51 for Vista(tested on Vista beta Build 5320)
10.USB 1.1 controller 1.03 for Win95 OSR2.1. 
11.M7101 Patch 1.01 for Win95. 
12.IRQ Miniport driver 0.1 for Windows95 
13.USB 2.0 controller 1.76 for Win98SE/WinME/Win2K/2003/WinXP.
14.M5228 v 5.0.2.8 driver for NT4/98se/Me/2000/XP/2003/x64
15.M5281 v 5.0.2.8 driver for NT4/98se/Me v 5.0.2.9 for 2000/XP/2003/x64/Vista(tested on Vista beta Build 5320)
16.M5287 v 6.2.0.9 driver for 2000(WHQL)/2003/XP(WHQL)/x64(WHQL)/Vista(tested on Vista beta Build 5320) 
17.M5288 v 6.2.1.8 driver for 2000(WHQL)/2003(WHQL)/XP(WHQL)/x64(WHQL)/Vista(tested on Vista beta Build 5320) 
18.M5289 v 5.0.3.0 driver for NT4/98se/Me/2000(WHQL)/XP(WHQL)/2003/x64(WHQL)/Vista(tested on Vista beta Build 5320) 
19.M5461 v 5.0.1.0 (MS Inbox/function) driver for 2000_sp4 /XP/2003


This driver will detect the OS version and show the items of drivers 
you need to install. 

*************
 Setup Items
*************

  Users don't need to decide what driver should be installed before executing
this integrated driver, i.e. it will automatically decide what drivers need
to be installed in the process of installation. However, users might have the 
demand that don't want some drivers in this integrated driver to be installed 
by default. To achieve this purpose, you can edit the "Setup Items" block in the
text file "install.ini" to change the default setup items before executing this 
driver. For example, if you don't want IDE Cache driver to be installed, then 
you can edit "install.ini" as follows.

[Setup Items]
Setup_VISTA64AGP=N
Setup_VISTA64LAN=Y
setup_VISTA64M5455=Y
setup_VISTA64M5281=Y
setup_VISTA64M5228=Y
setup_VISTA64M5287=Y
setup_VISTA64M5288=Y
setup_VISTA64M5289=Y


Setup_VISTAAGP=Y
Setup_VISTA87AGP=Y
Setup_VISTALAN=Y
Setup_VISTAAudio=Y
Setup_VISTAM5455=Y
Setup_VISTAFIR=Y
setup_VISTAM5281=Y
setup_VISTAM5228=Y
setup_VISTAM5287=Y
setup_VISTAM5288=Y
setup_VISTAM5289=Y


Setup_x64AGP=N
Setup_x64LAN=Y
setup_x64M5455=Y
setup_x64M5281=Y
setup_x64M5228=Y
setup_x64M5287=Y
setup_x64M5288=Y
setup_x64M5289=Y


Setup_XPAGP=Y
Setup_XP87AGP=Y
Setup_XPLAN=Y
Setup_XPFIR=Y
Setup_XPUSB20=Y
Setup_XPAudio=Y
Setup_XPMS=Y
Setup_XPSD=Y
Setup_XPM5455=Y
Setup_XPM5461=Y
setup_XPM5281=Y
setup_XPM5228=Y
setup_XPM5287=Y
setup_XPM5288=Y
setup_XPM5289=Y


Setup_2000AGP=Y
Setup_200087AGP=Y
Setup_2000LAN=Y
Setup_2000FIR=Y
Setup_2000Audio=Y
Setup_2000MS=Y
Setup_2000SD=Y
Setup_2000USB20=Y
Setup_2000M5455=Y
Setup_2000M5461=Y
setup_2000M5281=Y
setup_2000M5228=Y
setup_2000M5287=Y
setup_2000M5288=Y
setup_2000M5289=Y


Setup_MEAGP=Y
Setup_ME87AGP=Y
Setup_MEIDECache=N
Setup_MEFIR=Y
Setup_MEAudio=Y
Setup_MELAN=Y
Setup_MEMiniIDE=N
Setup_MEMS=Y
Setup_MESD=Y
Setup_MEUSB20=Y
Setup_MEM5455=Y
Setup_MEM5461=Y
setup_MEM5281=Y
setup_MEM5228=Y
setup_MEM5289=Y


Setup_98AGP=Y
Setup_9887AGP=Y
Setup_98IDECache=N
Setup_98FIR=Y
Setup_98Audio=Y
Setup_98MiniIDE=N
Setup_98MS=Y
Setup_98SD=Y
Setup_98LAN=Y
Setup_98USB20=Y 
Setup_98M5455=Y
Setup_98M5461=Y
setup_98M5281=Y
setup_98M5228=Y
setup_98M5287=N
setup_98M5289=Y


setup_NTM5281=Y
setup_NTM5228=Y
setup_NTM5289=Y

****************
 Default Status
****************

  The default status of the checkbox of setup items can be modified by editing
the "Default Status" block in the text file "install.ini". 

VISTA64_EnableAGP=N
VISTA64_EnableLAN=Y
VISTA64_EnableM5455=Y
VISTA64_EnableM5281=Y
VISTA64_EnableM5228=Y
VISTA64_EnableM5287=Y
VISTA64_EnableM5288=Y
VISTA64_EnableM5289=Y

VISTA_EnableAGP=N
VISTA_Enable87AGP=N
VISTA_EnableLAN=Y
VISTA_EnableAudio=Y
VISTA_EnableFIR=Y
VISTA_EnableM5455=Y
VISTA_EnableM5281=Y
VISTA_EnableM5228=Y
VISTA_EnableM5287=Y
VISTA_EnableM5288=Y
VISTA_EnableM5289=Y

x64_EnableAGP=N
x64_EnableLAN=Y
x64_EnableUSB20=N
x64_EnableM5455=Y
x64_EnableM5228=Y
x64_EnableM5281=Y
x64_EnableM5287=Y
x64_EnableM5288=Y
x64_EnableM5289=Y


XP_EnableAGP=Y
XP_Enable87AGP=Y
XP_EnableLAN=Y
XP_EnableFIR=Y
XP_EnableUSB20=N
XP_EnableAudio=Y
XP_EnableMS=N
XP_EnableSD=N
XP_EnableM5455=Y
XP_EnableM5461=N
XP_EnableM5281=Y
XP_EnableM5228=Y
XP_EnableM5287=Y
XP_EnableM5288=Y
XP_EnableM5289=Y


2000_EnableAGP=Y
2000_Enable87AGP=Y
2000_EnableLAN=Y
2000_EnableFIR=Y
2000_EnableAudio=Y
2000_EnableMS=Y
2000_EnableSD=Y
2000_EnableUSB20=Y
2000_EnableM5455=Y
2000_EnableM5461=N
2000_EnableM5281=Y
2000_EnableM5228=Y
2000_EnableM5287=Y
2000_EnableM5288=Y
2000_EnableM5289=Y


ME_EnableAGP=Y
ME_Enable87AGP=Y
ME_EnableIDECache=N
ME_EnableFIR=Y
ME_EnableAudio=Y
ME_EnableLAN=Y
ME_EnableMiniIDE=N
ME_EnableMS=Y
ME_EnableSD=Y
ME_EnableUSB20=Y
ME_EnableM5455=Y
ME_EnableM5461=Y
ME_EnableM5281=Y
ME_EnableM5228=Y
ME_EnableM5289=Y


98_EnableAGP=Y
98_Enable87AGP=Y
98_EnableIDECache=N
98_EnableFIR=Y
98_EnableAudio=Y
98_EnableMiniIDE=N
98_EnableMS=N
98_EnableSD=N
98_EnableLAN=Y
98_EnableUSB20=Y
98_EnableM5455=Y
98_EnableM5281=Y
98_EnableM5228=Y
98_EnableM5289=Y


NT4_EnableM5228=N
NT4_EnableM5281=N
NT4_EnableM5289=N


****************
 IP Enable
****************

EnableAGP=Y
EnableIDECache=N
EnableFIR=Y
EnableMiniIDE=N
EnableUSB=N
EnableM7101=N
EnableIRQ=N
EnableMS=Y
EnableAudio=Y
EnableSD=Y
Enable87AGP=Y
EnableLAN=Y
EnableUSB20=Y
EnableM5455=Y
EnableM5461=Y
EnableM5281=Y
EnableM5228=Y
EnableM5287=Y
EnableM5288=Y
EnableM5289=Y

  
**********************************
 (I)  ULi AGP Driver Version 2.20
**********************************

---------------
1. INTRODUCTION
---------------

  This file contains a variety of information you should read before 
installing ULi AGP drivers. This setup program contains three drivers, 
AgartD.VXD, ALiPCIMP.PCI and ALiAGP.sys. AgartD.VXD is the graphics 
address remapping table(GART) management for ULi chipsets at Windows 95.
ALiPCIMP.PCI is the PCI miniport driver providing PCI miniport
services at Windows 98/98SE. ALiAGP.sys is the PCI miniport driver 
providing PCI miniport services for Windows 2000 
 Windows XP.

----------------------
2. SYSTEM REQUIREMENTS
----------------------

Windows 95:
  1. Microsoft Windows 95 OSR2.1 or later version
  2. ALi AGP Driver 
  3. AGP VGA Card with Driver
  4. Direct X5 or above

Windows 98/98SE/ME:
  1. Microsoft Windows 98/98SE
  2. ULi AGP Driver 
  3. AGP VGA Card with Driver

Windows 2000:
  1. Microsoft Windows 2000(build 2195) or later version
  2. ULi AGP Driver 
  3. AGP VGA Card with Driver

Windows XP:
  1. Microsoft Windows XP(build 2600) or later version
  2. ULi AGP Driver 
  3. AGP VGA Card with Driver

Windows x64:
  1. Microsoft Windows x64 or later version
  2. ULi AGP Driver 
  3. AGP VGA Card with Driver

  
------------------------------
3. UNINSTALLATION INSTRUCTIONS
------------------------------

  1. Open "Control Panel" folder
  2. Invoke "Add\Remove Programs" icon
  3. Choose "ULi AGP Driver" item 
  4. Click on "Add/Remove" button to remove drivers.


*************************************  
 (II) ULi IDE Cache and Utility 1.06
*************************************

---------------
1. INTRODUCTION
---------------

 ULi IDE Cache and Utility 1.06 is a driver about IDE device read ahead control. this 
driver is for Windows 95/Windows 98/Windows 98SE and Windows Millennium. 
  When read-ahead is enabled, the cache controller module will accordding to current
read-ahead buffer size and cache frequency access your hard disk to speed up access
performance. In fact, IDE Cache Control Center will automatically determine when to 
read ahead data to cache memory according to current disk read status. The size of 
read-ahead data buffer and read-ahead frequency can be optionally changed by ULi IDE
Cache Control Center depends on the need of users. The disk access frequency for big 
files or large continuous disk sectors is directly proportional to setting read-ahead 
buffer. In contrast, if small files or big files with discontinuous disk sectors were 
accessed often, you can set read-ahead buffer to be less to reduce useless data being 
read to cache memory. 
  The default setting is the biggest read-ahead buffer size and the highest cache 
frequency.

----------------------
2. SYSTEM REQUIREMENTS
----------------------
Windows 95:
  1. Microsoft Windows 95 OSR2.0 or later version.
  2. ULi Cache driver (alivxd.vxd).
Windows 98/98SE:
  1. Microsoft Windows 98/98SE.
  2. ULi Cache driver (alivxd.vxd).
Windows Millennium:
  1. Microsoft Windows ME
  2. ULi Cache driver (alivxd.vxd).    
  
------------------------------
3. Uninstallation Instructions
------------------------------
Windows 95 and Windows 98/98SE/ME:
  1. Open "Control Panel" folder
  2. Invoke "Add\Remove Programs" icon
  3. Choose "ULi IDE Utility" item 
  4. Click on "Add/Remove" button to remove drivers.

------------------------
4. IDE Set Mode Utility
------------------------
  This utility is used to show device timing mode as PIO, DMA, or Ultra DMA.


*************************************************************************
 (III)  ULi FIR Driver Version 1.150(Win98SE),1.141(WinME),2.01(Win2000/WinXP) 
**************************************************************************

----------------
1. INTRODUCTION
----------------

  This driver supports ULi Fast Infrared Controller under Windows 98 SE,  Windows ME 
and Windows 2000/XP.  

----------------------
2. SYSTEM REQUIREMENTS
----------------------

(Windows 98 SE & Windows ME)    
 
1. Install ULi FIR Driver     - Run the setup program.   - This program will copy driver 
   files into your Windows system, then restart your computer.  
2. After system reboot, Windows will find the new hardware "ULi Fast Infrared Controller" 
   and install the driver.  
3. Restart the computer again to complete the installation.    

(Windows 2000 & WinXP)	  

1. Install ULi FIR Driver     - Run the setup program.     - This program will install 
   and load the driver and you don't have to reboot the computer.
  
------------------------------
3. UNINSTALLATION INSTRUCTIONS
------------------------------

  1. Open "Control Panel" folder.  
  2. Invoke "Add\Remove Programs" icon.  
  3. Choose "ULi FIR Driver" item.  
  4. Click on "Add/Remove" button to remove drivers.


******************************************************************************
 (IV) ULi Audio M5451 WDM Driver for Win98/Win98 SE/WinME/Win2000/WinXP
******************************************************************************

------------
INTRODUCTION
------------
This driver supports ULi M5451 PCI Audio Accelerator
integrated in ULi M1535/M1535D/M1535+/M1535D+ South Bridge.
  
 
------------------------------
1. Uninstallation Instructions
------------------------------
  * Uninstall from Add/Remove Programs
(This method is recommended if driver is previously installed by Setup program.)
1. Start Add/Remove Programs from Control Panel.
2. Select "ULi Audio Accelerator WDM Driver" item.
3. Click on "Remove" button.

* Uninstall from Device Manager
1. Start Device Manager from Control Panel's System applet.
2. Right click on "ULi Audio Accelerator WDM Driver" item, then
   select "Remove" (or "Uninstall") item from the popup menu.


--------------------------
2. ULi Sound Setup Utility
--------------------------
* From Control Panel window, double chick on the "ULi Sound Setup" applet
  icon to launch this program.

* MIDI Configuration
- Click on the "Sample" tab.
- "Sample Set" and "Sample Rate": select to determine a wavetable for ULi MIDI device.
- Press [OK] button and restart Windows to make these settings take effect
  on the next Windows session.
NOTES:
- These MIDI settings are meaningful only when system uses ULi Wavetable MIDI 
  device. To use ULi Wavetable MIDI device, execute Multimedia applet
  in Control Panel window, then from the MIDI tab, select "ULi Wavetable MIDI" 
  as the MIDI output device, in stead of "Microsoft GS Wavetable SW Synth".
- The alternative of Sample Set settings, 1MB, 4MB, or 8MB, represents the size of
  various ULi wavetable sample files. The larger wavetable sample file can provide
  better quality of MIDI sound, and consume more system resources (CPU computing
  and memory usage).
  Or user can select DLS option to use the GM.dls sample file provided by Microsoft.

* CODEC Power Saving Configuration
- "Power Management" tab
- "Enable Power Management" checkbox:
	to enable or disable CODEC power saving function
- "Always"/"Only in battery power mode" combobox:
	to select the active time of CODEC power saving function
- "Turn off CODEC power after (when no sound is played)" combobox:
	to set the idle time to automatically power down CODEC (PR0:ADC, PR1:DAC)
- "Enable External Amplifier Power Down":
	to further power down CODEC (PR2:Mixer, PR7:EAPD)
- [Apply] button: to apply the new settings,
- [OK] button: to apply the the new settings and exit program

-------------------
3. Driver File List
-------------------
* ALiADWDM.sys
  - is the driver binary
  - will be installed to %windir%\System32\Drivers
* ALiPanel.cpl
  - is the ULi Sound Setup Utility binary
  - will be installed to %windir%\System (in 98/ME) or System32 (in 2000/XP)
* ALiSndMg.exe
  - is the helper background process for CODEC power saving function
  - will be installed to %windir%\System
  - only is used in 98/ME
* ALi*.inf
  - will be installed to %windir%\inf (in 2000/XP)
    or inf\Other (in 98/ME)


================================================================
(V)  ULi Audio M5455 WDM Driver for Windows 98SE/ME/2000/XP
================================================================

------------
INTRODUCTION
------------
This driver supports ULi M5455 PCI Audio integrated in ULi M1563 South Bridge.

------------------------------
1. Uninstallation Instructions
------------------------------
* Uninstall from Add/Remove Programs
(This method is recommended if driver is previously installed by Setup program.)
1. Start Add/Remove Programs from Control Panel.
2. Select "ULi M5455 Audio Controller" item.
3. Click on "Remove" button.

* Uninstall from Device Manager
1. Start Device Manager from Control Panel's System applet.
2. Right click on "ULi M5455 Audio Controller" item, then
   select "Remove" (or "Uninstall") item from the popup menu.

--------------------------
2. ULi Sound Setup Utility
--------------------------
* From Control Panel window, double chick on the "ULi Sound Setup" applet
  icon to launch this program.

* CODEC Power Saving Configuration
- "Power Management" tab
- "Enable Power Management" checkbox:
	to enable or disable CODEC power saving function
- "Always"/"Only in battery power mode" combobox:
	to select the active time of CODEC power saving function
- "Turn off CODEC power after (when no sound is played)" combobox:
	to set the idle time to automatically power down CODEC (PR0:ADC, PR1:DAC)
- "Enable External Amplifier Power Down":
	to further power down CODEC (PR2:Mixer, PR7:EAPD)
- [Apply] button: to apply the new settings,
- [OK] button: to apply the the new settings and exit program

-------------------
3. Driver File List
-------------------
* ALi55WDM.sys
  - is the driver binary
  - will be installed to %windir%\System32\Drivers
* ALi55CPL.cpl
  - is the ULi Sound Setup Utility binary
  - will be installed to %windir%\System (in 98/ME) or System32 (in 2000/XP)
* ALi55PRP.dll
  - the property page will display some AC97 codec features.
  - will be installed to %windir%\System (in 98/ME) or System32 (in 2000/XP)
* ALi*.inf
  - will be installed to %windir%\inf (in 2000/XP)
    or inf\Other (in 98/ME)    



********************************************************
(VI) ULi Memory Stick Driver for Windows 98SE/ME/2000/XP
********************************************************

--------------
1.INTRODUCTION
--------------
This driver supports ULi M5471 PCI to Memory Stick Controller.
------------------------------
2. Uninstallation Instructions
------------------------------
* Uninstall from Add/Remove Programs
(This method is recommended if driver is previously installed by Setup program.)
1. Start Add/Remove Programs from Control Panel.
2. Select "ULi Memory Stick driver" item.
3. Click on "Remove" button.

* Uninstall from Device Manager
1. Start Device Manager from Control Panel's System applet.
2. Right click on "ULi Memory stick Controller"  item,
   then select "Remove" (or "Uninstall") item from the popup menu.



***************************************************
(VII) ULi SD MMC Driver for Windows 98SE/ME/2000/XP
***************************************************

--------------
1.INTRODUCTION
--------------
This driver supports ULi M5473 PCI to Memory Stick Controller.

------------------------------
2. Uninstallation Instructions
------------------------------
* Uninstall from Add/Remove Programs
(This method is recommended if driver is previously installed by Setup program.)
1. Start Add/Remove Programs from Control Panel.
2. Select "ULi SD MMC Driver" item.
3. Click on "Remove" button.

* Uninstall from Device Manager
1. Start Device Manager from Control Panel's System applet.
2. Right click on "ULi SD/MMC Controller"  item,
   then select "Remove" (or "Uninstall") item from the popup menu.



***************************************************
(VIII) ULi LAN Driver for Windows 98SE/ME/2000/XP
***************************************************

--------------
1.INTRODUCTION
--------------
This driver supports ULi M5261/M5263 PCI Fast Ethernet Controller in ULi M1563 South Bridge & M1689 Bridge

------------------------------
2. Uninstallation Instructions
------------------------------
* Uninstall from Add/Remove Programs
(This method is recommended if driver is previously installed by Setup program.)
1. Start Add/Remove Programs from Control Panel.
2. Select "ULi LAN Driver " item.
3. Click on "Remove" button.

* Uninstall from Device Manager
1. Start Device Manager from Control Panel's System applet.
2. Right click on "ULi PCI Fast Ethernet Controller"  item,
   then select "Remove" (or "Uninstall") item from the popup menu.

***********************************************
 (IX) ULi Mini IDE Driver 1.51 for Win2000/XP
***********************************************

------------
INTRODUCTION
------------

This file contains a variety of information you should read before 
installing the ULi mini-IDE driver.  ULi mini-IDE is a mini driver 
for Windows 2000/Xp. It is compliant to Microsoft in-box driver to 
tune running mode when device or system is unstable. It also helps 
Microsoft in-box driver to enable DMA mode of ATAPI devices 
(CD, CD-RW, DVD...) for older ULi chips.


------------------------------
1. Uninstallation Instructions
------------------------------

Use control panel :
  1. Open "Control Panel" folder
  2. Invoke "Add/Remove Programs" icon
  3. Choose "ULi Mini IDE Driver" item 
  4. Click on "Change/Remove" button to remove driver.

-----------------------
2. IDE Set Mode Utility
-----------------------

This utility is used to set device timing mode as PIO, DMA, or Ultra DMA.
Its main purpose is to solve some device "compatibility" problems. 

For example, your CDROM drive reports its capability that it can run "DMA" 
and "PIO" timing mode.
Due to device firmware bug or some other reason, this device cannot work on DMA mode.
In this case, you can run "IDE Set Mode Utility" to set device timing mode as PIO.

The utility is in "Start->Programs->uLi Products->IDE Set Mode Utility".

After you run it, you can use its default setting with "Auto" checked.
When "Auto" is checked, device will run its best timing mode.

In this case, if you want to change device timing mode as PIO, you can uncheck "AUto"
item and then move mouse cursor to click on slider bar, draw it to "PIO".
After you change timing mode and click "OK", you will be notified to "Restart" your 
system for this new setting to work.

You can control each device to run at different timing mode by clicking on "DEV0", "DEV1"
, "DEV2" and "DEV3".

When "Auto" is checked, device will run its best timing mode. 
When "Auto" is unchecked, you can move mouse cursor to click on slider bar, draw it to 
different timing mode like "PIO", "DMA", "UDMA33", "UDMA66", "UDMA100/133".

"Running Mode" means the current timing mode of the selected device (DEV0/DEV1/DEV2/DEV3).


**********************************************
 (X)  ULi USB Controller 1.03 for Win95 OSR2.1
**********************************************

--------------
1.INTRODUCTION
--------------
This program is used to solve the incorrect identification of 
ULi USB Host Controller under Windows 95 OSR2.1. You should 
update to Windows 95 OSR2.1 with Microsoft usbsupp.exe before 
executing this program. Be careful the language of usbsupp.exe
or it will damage your system.

----------------------
2. SYSTEM REQUIREMENTS
----------------------
1.Windows 95
  MS Windows 95 users can execute USBSUPP.EXE (provided by Microsoft)
  to update OSR2.0 to version 2.1.
  We can get this file from Microsoft (www.microsoft.com).

2.Windows 98:
  Microsoft has the driver for USB in Windows98, so this
  program is not necessary if your operating system is 
  Windows 98 or later.



**********************************************
 (XI)  ULi M7101 Patch Version 1.01 for Win95 
**********************************************

--------------
1.INTRODUCTION
--------------
There will has a "!" mark at device manager under Win95 when ULi M7101 is
available in the system. The "!" mark let user has some suspicion of system'
s configuration. This is because Win95 can not recognize the M7101 device.
This patch provide a easy install/uninstall utility to put the ULi M7101
information into Win95 database.

----------------------------
2.Installation Instructions
----------------------------
Windows 95:
  1. Install Windows 95 OSR2 or later version
  2. Upgrade Windows 95 to version OSR2.1 by running USBSUPP.EXE.
     We can get this file from Microsoft (www.microsoft.com).

Windows 98:
     For Win98,WinMe or WinNT,the utility will do nothing.

**********************************************
 (XII)   ULi IRQ Miniport Driver Version 0.1 for Win95
**********************************************

--------------
1.INTRODUCTION
--------------
This program support IRQ Routing function in Windows 95.

----------------------------
2.Installation Instructions
----------------------------
Windows 95:
  1. Install Windows 95 OSR2 or later version
  2. Upgrade Windows 95 to version OSR2.1 by running USBSUPP.EXE.
     We can get this file from Microsoft (www.microsoft.com).
Windows 98:
     For Win98,WinMe or WinNT,the utility will do nothing.



**********************************************
 (XIII)   USB 2.0 Controller driver
**********************************************

----------------
 INTRODUCTION
----------------

  This driver supports ULi EHCI host Controller under Windows 98 SE,  Windows ME , Windows 2000
  and Windows XP.  
----------------------------
1. Installation Instructions
----------------------------

(Windows 98 SE & Windows ME)
A.When ULi USB 2.0 Controller has attached on system 
  This program will copy driver files into your Windows system,and then system will
       show a dialog to warn user that system will install "Windows hardfix UPDATE"
       Please click "Yes" to continue install,then restart your computer.
   
B.If no ULi USB 2.0 Controller on system
     This program will copy driver files into your Windows system and then system will
       show a dialog to warn user that system will install "Windows hardfix UPDATE"
       Please click "Yes" to continue install, then turn off your computer.
     - Attach ULi USB 2.0 Controller card on your system and then reboot your computer.
     - After system reboot, Windows will find the new hardware "ULi PCI to USB Enhanced
       Host Controller" and install the driver.
  
 
(Windows 2000)	
A.When ULi USB 2.0 Controller has attached on system 
      Run the setup program.
     
B.If no ULi USB 2.0 Controller on system
      Run the setup program.
     

 (Windows XP)
A.When ULi USB 2.0 Controller has attached on system  
  1. Install ULi USB2.0 Driver
    - After install ULi USB 2.0 driver successfully. System will detect "USB 2.0 Root
        Hub". Please select "install the software automatically (Recommended)" and then 
        click "Next" button to continue install.
    
    
B.If no ULi USB 2.0 Controller on system
    This program will copy driver files into your Windows system, then turn off 
      your computer.
      Attach ULi USB 2.0 Controller card on your system and then reboot your computer.
    - After system reboot, Windows will find the new hardware "ULi PCI to USB Enhanced
     Host Controller" 
    - After install ULi USB 2.0 driver successfully. System will detect "USB 2.0 Root
      Hub". Please select "install the software automatically (Recommended)" and then 
      click "Next" button to continue install.
    
     

  Notice:
  If you can't setup driver successfully. Please reboot your system and then follow 
  above steps to install driver again.
   
 ------------------------------
 2. Uninstallation Instructions
 ------------------------------

  1. Open "Control Panel" folder.
  2. Invoke "Add\Remove Programs" icon.
  3. Choose "ULi USB2.0 Driver" item.
  4. Click on "Add/Remove" button to remove drivers.


==============================================================================
(xIIII)  ULi Audio M5461 Azalia Driver for Windows 2000 2000_sp4 /XP_SP1 /2003
==============================================================================
--------------
 INTRODUCTION
--------------
  This driver is Microsoft inbox driver.
  This driver supports ULi Azalia Audio Controller under Windows 2000_SP4 and Windows XP_sp1 or later version
  , and Windows2003 32bit.


***********
Change List   
***********
v2.20
1.Update setup package to support Vista(tested on Vista beta Build 5320)
2.Update ULi M5288 v6.2.1.8 driver support for 2000/XP/2003/x64/Vista(tested on Vista beta Build 5320) 
3.Update ULi Lan driver v3.51 driver for Vista(tested on Vista beta Build 5320). 
v2.13
1.Update ULi M5287 v6.2.0.9 driver logo'd for 2000/XP/x64
2.Update ULi M5288 v6.2.1.3 driver support Raid 5 function for 2000/XP/2003/x64 

v2.12
1.Update ULi USB 2.0 Host Controller driver to 1.76
v2.11
1.Update ULi M5287 v6.2.0.8 driver for 2000/XP
2.Update ULi M5288 v6.2.0.8 driver for 2000/XP
v2.1
1.Update ULi M5287 v6.2.0.7 driver logo'd for 2000/XP
2.Update ULi M5288 v6.2.0.7 driver logo'd for 2000/XP
3.Update ULi M5289 v5.0.3.0 driver logo'd for 2000/XP/x64
4.Update ULi M5287 v6.2.0.8 driver logo'd for WinXP x64
5.Update ULi M5288 v6.2.0.8 driver logo'd for WinXP x64
v2.0965
1.Update ULi M5287 v6.2.0.6 driver for 2000/2003/XP/x64
2.Update ULi M5288 v6.2.0.6 driver for 2000/2003/XP/x64
v2.0964
1.Update ULi M5287 inf file.
v2.0963
1.Update ULi M5287 from version 6.2.0.3 to 6.2.0.5 for 2000/2003/XP/x64
2.Update ULiRaid AP for M5289 SATA
v2.0962
1.Update ULi USB 2.0 Host Controller driver to 1.75
2.Update ULi AGP driver v2.30 logo'd to support AMD Dual Core CPU for WinXP/x64.

v2.096
1.Update ULi Lan driver v3.50 driver logo'd for XP64bit/XP/2K. 
2.Update ULI M5287/5289 driver logo'd for XP64bit. 
v2.095
1.Update ULi SD/MMC driver from 1.10.1030 to 1.10.1040 for Win2000/WinXP. 
2.Update ULi USB 2.0 Host Controller driver from version 1.72 to 1.73 for 98se/Me/2000/XP/2003
3.Update ULi LAN driver from version 3.12 to 3.40 for 98se/Me/2000/XP/2003/x64
4.Update ULi M5228 from version 5.0.2.7 to 5.0.2.8 for NT4/98se/Me/2000/XP/2003/x64
5.Update ULi M5281 from version 5.0.2.7 to 5.0.2.8 for NT4/98se/Me/2000/XP/2003/x64
6.Update ULi M5289 from version 5.0.2.7 to 5.0.2.9 for NT4/98se/Me/2000/XP/2003/x64 
7.Update ULi M5287 from version 6.1.0.2 to 6.2.0.3 for 2000/2003/XP/x64
8.Update ALi5289.exe for NT4/98se/Me/2000/XP/2003/x64 
9.Update JMAPP AP version 5.0.2.8 for M5281 SATA
10.Add ULiRaid AP for M5287 SATA

v2.094
1.Update txtsetup.oem
2.Add ULi M5287 cat file for XP

v2.093
1.Add items to determini to install SATA AP by install.ini
2.Update ULi USB 2.0 Host Controller driver from version 1.71 to 1.72.
3.Update ULi M5287 from version 6.0.0.0 to 6.1.0.0 for 2000/XP
4.Update ULi LAN driver from version 3.11 to version 3.12 

v2.092
1.Update txtsetup.oem

v2.091
1.Add ULi M5287 v 6.0.0.0 driver for 2000/XP

v2.09
1.Update ULi M1683/M1685/M1689 AGP driver from version 2.12 to 2.20 for x64/XP/2003 
  and from  2.12  to  2.13 for 98/Me
2.Update ULi LAN driver from version 3.01 to version 3.10 for XP/2003/x64 
  and from version 3.01 to version 3.11 for 2000/Me/98
3.Update ULi M5455 Audio Driver from 7005 to 7006 for xp/2003/2000/Me/98


v2.08
1.Update ULi M1683/M1685/M1689 AGP driver from version 2.10 to 2.12
2.Update ULi USB 2.0 Host Controller driver from version 1.19 to 1.70
3.Update ULi LAN driver from version 1.50 to version3.01 
4.Add ULi M5228 v 5.0.2.7 driver for NT4/98se/Me/2000/XP/2003/x64
5.Add ULi M5281 v 5.0.2.7 driver for NT4/98se/Me/2000/XP/2003/x64
5.Add ULi M5289 v 5.0.2.7 driver for NT4/98se/Me/2000/XP/2003/x64
6.Add ULi M5461 v 5.0.1.0 driver for 2000_sp4/XP_SP1/2003

V2.07
1.Update ULi M1683 AGP driver from version 2.01 to 2.10

3.Update ULi LAN driver from version 5.1.2600.0130 to version 5.1.2600.0150 for WinXP and
  from version 5.1.2600.0132 to version 5.0.2000.0150 for Win98SE/Me/2000.
4.Update ULi M1687 AGP driver from 8.04.2600 to 8.1.2.1 for Win98SE/WinME/Win2000/WinXP

v2.05
1.Update ULi AUDIO(M5451) WDM driver from version 5250 to 5260.
2.Update ULi USB 2.0 Host Controller driver from version 1.05 to 1.13.
3.Update ULi LAN driver from version 5.1.2600.0120 to version 5.1.2600.0130 for WinXP and
from version 5.1.2600.0120 to version 5.1.2600.0132 for Win98SE/Me/2000.

v2.04
1.Update ULi AGP driver from version 2.00 to 2.01.
2.Update ULi USB 2.0 Host Controller driver from version 1.03 to 1.05.
3.Update ULi Mini-IDE driver from 1.5.0.0  to 1.5.1.0 for Win2K/XP.

v2.03
1.Update ULi AUDIO(M5455) WDM driver from version 7004 to 7005.
2.Update ULi USB 2.0 Host Controller driver from version 1.02 to 1.03.
3.Update ULi FIR driver from version 1.26 for Win 2000 to 2.01 for Win 2000/XP. 
4.Replace ULi Ultra-IDE 4.0.0.7 with Mini-IDE 1.5.0.0 for Win2K/XP.

v2.02
1.Update ULi AGP driver from version 1.93 to 2.00.
2.Add AGP driver 8.04 for M1687 chipset in Win98SE/WinME/Win2000/WinXP.
3.Update ULi AUDIO(M5451) WDM driver from version 5220 to 5250.
4.Update ULi LAN driver from version 5.1.2600.0105 to version 5.1.2600.0120 for Win98SE/WinME
  /Win2000/WinXP.
5.Add ULi USB 2.0 Host Controller driver 1.02 for Win98SE/WinME/Win2000/WinXP.

v2.01
1.Update ULi AUDIO(M5455) WDM driver from version 7003 to 7004.
2.Update ULi Memory Stick driver from version 0601 to 1.32.1018 for Win98SE/WinME.
3.Update ULi Memory Stick driver from version 0801 to 1.32.1030 for Win2000/WinXP.
4.Update ULi SD MMC driver from version 0601 to version 1.10.1016 for Win98SE/WinME.
5.Update ULi SD MMC driver from version 0801 to version 1.10.1030 for Win2000/WinXP.
6.Update ULi LAN driver from version 0103 to version 5.1.2600.0105 for Win98SE/WinME
  /Win2000/WinXP.
7.Fix issue that M1681 chipset motherboard can't install AGP driver successfully.

v2.00
1.Update ULi AUDIO(M5451) WDM driver from version 5210 to 5220.
2.Support ULi AUDIO(M5455) WDM driver version 7003 for Win98SE/WinME/Win2000/WinXP.
3.Support ULi Memory Stick driver version 0601 for Win98SE/WinME
4.Support ULi Memory Stick driver version 0801 for Win2000/WinXP.
5.Support ULi SD MMC driver version 0601 for Win98SE/WinME.
6.Support ULi SD MMC driver version 0801 for Win2000/WinXP.
7.Support ULi LAN driver version 0103 for Win98SE/WinME/Win2000/WinXP.


v1.10
Update ULi AGP driver from version 1.91 to 1.93.

v1.091
1.Update ULi Ultra-IDE driver from 4.0.0.6 to 4.0.0.7.
  
v1.09
1.Update ULi AGP driver from version 1.90 to 1.91.
2.Update ULi AUDIO WDM driver from version 5181 to 5210.
3.Update ULi Ultra-IDE driver from 4.0.0.5 to 4.0.0.6.

V1.08
1.Update ULi AGP driver version 1.90 for Win98/ME with WHQL.
2.Fix Integrated driver issue that AGP driver can't install on win 98/98SE 
  for ULi M1672 north bridege.


V1.07
1.Update ULi AGP driver from version 1.81 to 1.90.
2.Update ULi AUDIO WDM driver from version 5170 to 5181.
3.Replace ULi Win200 Mini-IDE driver 1.41 with Ultra-IDE 4.0.0.5 for Win2K/XP.
4.Update ULi IDE Cache Utility driver from version 1.05 to 1.06
5.Update ULi FIR driver from version 1.141 for Win 98/98SE to 1.150.
6.Update ULi FIR driver from version 1.141 for Win 2000 to 1.26 for Win 2000/XP. 


V1.06
1.Update ULi AGP driver from version 1.80 to 1.81.
2.Update ULI AUDIO WDM driver from version 5140 to 5170. 

V1.05
1.Support ULi AGP driver 1.80 for Win95 OSR2.1/Win98/Win98SE/WinME/Win2000/WinXP
2.Support ULi AUDIO WDM driver 5140 for Win98/Win98SE/WinME/Win2K
3.Support ULi IDE Cache Utility 1.05 for Win95 OSR2.1/Win98/Win98SE/WinME
4.Support ULi Mini-IDE driver 1.41 for Win2K
5.Support ULi FIR driver 1.141 for Win98/Win98SE/WinME/Win2K
6.Support ULi USB Controller 1.03 for Win95 OSR2.1.
7.Support ULi IRQ Miniport driver 0.1 for Win95.
8.Support ULi M7101 Patch 1.01 for Win95.



ULi Corporation (ULi) web sites:
  http://www.Uli.com.tw/ (Taiwan)
 
